For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Gently pry up on the sun sensor to remove it.
3. Secure the electrical connector to prevent it from falling beneath the dash.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Insert and press the sun sensor into position in the dash.
3. Connect the negative battery cable.