For 1990-2009 cars

#### Tools Required

J 26610 Installer

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
4. Remove the dust boot retaining clamps.
5. Remove the dust boot.

### Installation Procedure

1. Install the dust boot.
2. Install the tie rod end dust boot retaining clamp.
3. Install the cylinder end dust boot retaining clamp with the J 26610 .
4. Install the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
5. Install the wheel. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.