For 1990-2009 cars

### Removal Procedure

1. Remove the air filter housing.
2. Disconnect the shift control cable from the selector lever and the control cable bracket.
3. Remove the shift control cable bracket bolts and the bracket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the shift control cable bracket bolts and the bracket and tighten to 25 N·m (18 lb ft).
2. Connect the shift control cable to the selector lever and the control cable bracket.
3. Install the air filter housing.