For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.
2. Pry off the vents by inserting a screwdriver.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Press the vents onto the housing and tighten the vent screws to 3 N·m (27 lb in).
2. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.