For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the lower steering column cover panel screw.
3. Turn the steering wheel in order to expose the upper steering column cover panel screws.
4. Remove the upper steering column cover panel screws.
5. Remove the upper and the lower steering column cover panels.
6. Remove the turn signal switch by pushing in on the tabs on the top and the bottom of the switch housing.
7. Disconnect the electrical connectors from the turn signal switch.

### Installation Procedure

1. Connect the electrical connectors to the turn signal switch.
2. Install the turn signal switch by snapping the switch into the switch housing.
3. Install the upper and the lower steering column cover panels.
4. Turn the steering wheel in order to expose the upper steering column cover panel screw holes.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the upper and the lower steering column cover panel screws and tighten to 1.5 N·m (13 lb in).
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.