For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat backs.
2. Remove the retaining clips and reposition the rear seat back cover.
3. Remove the nuts and the armrest.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the armrest with the nuts and tighten to 24 N·m (18 lb ft).
2. Install the rear seat back backside cover with the retaining clips.
3. Raise and secure the rear seat backs in the upright position.