For 1990-2009 cars

### Removal Procedure

1. Remove the audio system trim plate.
2. Remove the screws and the instrument cluster trim panel.
3. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the instrument cluster trim panel with the screws.

Tighten
Tighten the instrument cluster trim panel screws to 3 N·m (27 lb in).

3. Install the audio system trim plate.