For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement .
3. Remove the screws and the front door lock.
4. Disconnect the lock rods.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Connect the lock rods.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front door lock with the screws.

Tighten
Tighten the front door lock screws to 8 N·m (71 lb in).

4. Install the seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement .
5. Connect the negative battery cable.