For 1990-2009 cars

### Removal Procedure

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

1. Raise and suitably support the vehicle.
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the front mud guard. Refer to Rear Mud Flap Guard Replacement .
4. Remove the screws and the front wheel well splash shield.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the screws and the front wheel well splash shield.

Tighten
Tighten the front wheel well splash shield screws to 2 N·m (18 lb in).

2. Install the front mud guard. Refer to Rear Mud Flap Guard Replacement .
3. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.