For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheels.
3. Remove the rear strut lower nut-to-knuckle.
4. Remove the rear seat and rear strut upper nut-to-body. Refer to Rear Seat Back Cushion Hinge Replacement.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear strut with upper nut-to-body and rear seat and tighten to 50 N·m (37 lb ft). Refer to Rear Seat Back Cushion Hinge Replacement.
2. Install the rear strut with lower nut-to-knuckle and tighten to 90 N·m (66 lb ft).