For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the ignition coil wiring harness connectors.
3. Remove the ignition coils.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the ignition coils.

Tighten
Tighten the ignition coil retaining bolts to 7 N·m (62 lb in).

2. Connect the ignition coil wiring harness connectors.
3. Connect the negative battery cable.