For 1990-2009 cars

### Removal Procedure

1. Remove the audio system trim plate.
2. Remove the screws and the instrument cluster trim panel.
3. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the instrument cluster trim panel with the screws and tighten to 3 N·m (27 lb in).
3. Install the audio system trim plate.