For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front bumper fasica extension, if equipped. Refer to Front Bumper Fascia Extension Replacement.
3. Remove the front wheel well splash shields. Refer to Wheelhouse Splash Shield Replacement.
4. Remove the turn signal lamps, the front side marker lamps, the fog lamps, and the headlamps.
5. Remove the fender-to-fascia bolts and the screws.
6. Remove the lower fascia screws and the bolts.
7. Remove the upper fascia screws.
8. Remove the front bumper fascia.

### Installation Procedure

1. Install the front bumper fascia.
2. Install the upper fascia screws.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the lower fascia screws and the bolts. Tighten the bolts to 2 N·m (18 lb in).
4. Install the fender-to-fascia bolts and the screws.

• | Tighten the fender-to-fascia bolts to 10 N·m (89 lb in).

• | Tighten the fender-to-fascia screws to 4 N·m (36 lb in).

5. Install the headlamps, the front side marker lamps, the fog lamps, and the turn signal lamps.
6. Install the front wheel well splash shields. Refer to Wheelhouse Splash Shield Replacement.
7. Install the front bumper fasica extension, if removed. Refer to Front Bumper Fascia Extension Replacement.
8. Connect the negative battery cable.