For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Clutch Housing-to-Transaxle Housing Bolts | 20-25 N·m | 15-18 lb ft
Concentric Slave Cylinder to Clutch Oil Pipe Screw | 16 N·m | 12 lb ft
Concentric Slave Retaining Bolts | 8-12 N·m | 71-106 lb in
Fluid Drain Plug | 6 N·m + 45-180° | 53 lb in + 45-180°
Fluid Level Check Plug | 6 N·m + 45-180° | 53 lb in + 45-180°
Front Damper Bush Mounting Bolts | 50 N·m | 37 lb ft
Input Shaft Retainer Plug | 120-130 N·m | 89-96 lb ft
Interm Shaft Retainer Plug | 90-100 N·m | 66-74 lb ft
Left Lower Engine-to-Transaxle Bolts (2.0 S Diesel) | 75 N·m | 55 lb ft
Left Lower Engine-to-Transaxle Bolts (HFV6 3.2L) | 50 N·m | 37 lb ft
Left Upper Transaxle Mounting Bracket Bolts | 50 N·m | 37 lb ft
Oil Pan Flange-to-Transaxle Bolts | 50 N·m | 37 lb ft
Output Shaft Retainer Plug | 120-130 N·m | 89-96 lb ft
Rear Transaxle Mounting Bracket Bolts | 90 N·m | 66 lb ft
Right Lower Engine-to-Transaxle Bolts (FAM II 2.4D or 2.0S Diesel) | 75 N·m | 55 lb ft
Right Lower Engine-to-Transaxle Bolt (HFV6 3.2L) | 50 N·m | 37 lb ft
Shift Control Cable Bracket Bolts | 15-20 N·m | 11-15 lb ft
Shift Control Lever Housing Bolt | 8 N·m | 71 lb in
Shift Guide Bolt | 20-25 N·m | 15-18 lb ft
Shift Retaining Bolts | 20-25 N·m | 15-18 lb ft
Thread Pin | 6-9 N·m | 53-80 lb in
Transaxle Housing-to-Clutch Housing Bolts | 20-25 N·m | 15-18 lb ft
Transaxle Housing Rear Cover Bolts | 20-25 N·m | 15-18 lb ft
Upper Transaxle-to-Engine Retaining Bolts (FAM II 2.4D or 2.0S Diesel) | 75 N·m | 55 lb ft
Upper Transaxle-to-Engine Bolt (HFV6 3.2L) | 50 N·m | 37 lb ft