For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
3. Disconnect the electrical connector.
4. Remove the screws and the glass antenna module.

### Installation Procedure

1. Install the glass antenna module with the screws.
2. Connect the electrical connectors.
3. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
4. Connect the negative battery cable.