For 1990-2009 cars

### Removal Procedure

1. Open the luggage compartment lid.
2. Remove the weatherstrip from around the gutter.

### Installation Procedure

1. Install the weatherstrip onto the gutter flange.
2. Inspect the weatherstrip. Make sure that the clinch is completely seated onto the flange.
3. Using a water hose without a nozzle, test the rear deck lid to make sure that no leaks are present.

• | If there are no leaks present, no further repair is required.

• | If leaks are present, continue with the remainder of the installation procedure.

4. Remove the weatherstrip.
5. Install the new weatherstrip onto the gutter flange.