For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the oil filter.
3. Remove the oil filter adapter retaining bolts and oil filter adapter.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil filter adapter.

Tighten
Tighten the oil filter adapter retaining bolts to 23 N·m (17 lb ft).

2. Install the oil filter

Tighten
Tighten the oil filter to 14 N·m (124 lb in).