For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back and the rear seat cushion. Refer to Rear Split Folding Seat Back Replacement or Rear Seat Cushion Replacement.
2. Remove the bolts and the seat back center hinge.
3. Remove the rear seat bolster cushion. Refer to Seat Back Cushion Side Bolster Panel Replacement.
4. Remove the volts and the seat back outer hinge.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat back outer hinge with the bolts and tighten to 12 N·m (106 lb in).
2. Install the rear seat side bolster cushion. Refer to Seat Back Cushion Side Bolster Panel Replacement.
3. Install the seat back center hinge with the bolts and tighten to 12 N·m (106 lb in).
4. Install the rear seat back and the rear seat cushion. Refer to Rear Split Folding Seat Back Replacement or Rear Seat Cushion Replacement.