For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat backs.
2. Remove the retaining clips and reposition the rear seat back backside cover.
3. Remove the nuts, the bolts, and the seat back from the hinges.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat back to the hinges with the bolts and the nuts.

#### Tighten

• | Tighten the rear seat back bolts to 25 N·m (18 lb ft).

• | Tighten the rear seat back nuts to 25 N·m (18 lb ft).

2. Install the rear seat back backside cover with the retaining clips.
3. Raise and secure the rear seat back in the upright position.