For 1990-2009 cars

### Removal Procedure

1. Lower the window completely.
2. Remove the outside channel molding screw.
3. Remove the outside rearview mirror. Refer to Power Mirror Replacement.
4. Lift the outside channel molding off the door.

### Installation Procedure

1. Press the outside channel molding onto the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the outside channel molding screw.

Tighten
Tighten the outside channel molding screw to 1.3 N·m (12 lb in).

3. Install the outside rearview mirror. Refer to Power Mirror Replacement.
4. Raise the window.