For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the dust cover from the under body of the vehicle.
3. Remove the power steering pipe fixing bolts.
4. Remove the centermember front damping block bolt and rear damping block bolt.
5. Remove the centermember bolts and remove the centermember assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the centermember assembly and bolts.

Tighten
Tighten the centermember bolts to 90 N·m (66 lb ft).

2. Install the centermember front damping block bolt and rear damping block bolt.

Tighten
Tighten the centermember front damping block bolt and rear damping block bolt to 80 N·m (59 lb ft).