For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement.
3. Remove the defective bulb from the rear of the cluster.

### Installation Procedure

1. Install the new bulb.
2. Install the instrument cluster. Refer to Instrument Cluster Replacement.
3. Connect the negative battery cable.