For 1990-2009 cars

## Brake Pressure Modulator Valve Assembly Replacement Except V275

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the cooling surge tank. Refer to Radiator Surge Tank Replacement .
3. Disconnect the ABS wiring harness connector (2) from the socket on the electronic brake control module (EBCM).
4. Cover the connector and the socket with shop cloths to protect it from the brake fluid.

Important: Do not allow air from the master cylinder into the hydraulic unit or the brake pipes. If air gets into the hydraulic unit, perform a bleeding procedure using a scan tool programmed for the ABS system. As long as no air enters the hydraulic unit, a simple bleeding procedure is all the system will require.

5. Remove the 6 brake pipe fitting nuts from the hydraulic unit.
6. Remove the mounting bracket bolts from the brake modulator assembly.
7. Remove the brake modulator assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 6 brake pipe fitting nuts.

Tighten
Tighten the nuts to 16 N·m (12 lb ft).

2. Install the brake modulator assembly and secure with the mounting bracket bolts (2).

Tighten
Tighten the bolts to 22 N·m (16 lb ft).

3. Connect the ABS wiring harness (2).

Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

4. Inspect the fluid level of the brake master cylinder. Add new brake fluid as required.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
6. Test the brake system for leaks.
7. Install the cooling surge tank. Refer to Radiator Surge Tank Replacement .
8. Connect the negative battery cable.
9. Refer to Control Module References for programming and setup information.

## Brake Pressure Modulator Valve Assembly Replacement V275

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement or Air Cleaner Assembly Replacement.
3. Disconnect the ABS wiring harness connector (1) from the socket on the electronic brake control module (EBCM).
4. Cover the connector and the socket with shop cloths to protect it from the brake fluid.

Important: Do not allow air from the master cylinder into the hydraulic unit or the brake pipes. If air gets into the hydraulic unit, perform a bleeding procedure using a scan tool programmed for the ABS system. As long as no air enters the hydraulic unit, a simple bleeding procedure is all the system will require.

5. Remove the 6 brake pipe fitting nuts from the hydraulic unit.
6. Remove the mounting bracket bolts (1) from the brake modulator assembly.
7. Remove the brake modulator assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 6 brake pipe fitting nuts.

Tighten
Tighten the nuts to 16 N·m (12 lb ft).

2. Install the brake modulator assembly and secure with the mounting bracket bolts (1).

Tighten
Tighten the bolts to 11 N·m (8 lb ft).

3. Connect the ABS wiring harness (1).

Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

4. Inspect the fluid level of the brake master cylinder. Add new brake fluid as required.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
6. Test the brake system for leaks.
7. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement or Air Cleaner Assembly Replacement.
8. Connect the negative battery cable.
9. Refer to Control Module References for programming and setup information.