For 1990-2009 cars

### Removal Procedure

1. Remove the kick panel, the front rocker panel, and the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
2. Remove the front door opening weatherstrip.

### Installation Procedure

1. Install the front door opening weatherstrip.
2. Install the kick panel, the front rocker panel, and the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .