For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the off position.
2. Disconnect the electronic throttle control (ETC) connector from the accelerator pedal.
3. Remove the 3 accelerator pedal retaining bolts.
4. Remove the accelerator pedal.

### Installation Procedure

1. Position the accelerator pedal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 3 accelerator pedal retaining nuts.

Tighten
Tighten the upper accelerator pedal retaining bolts to 10 N·m (89 lb in).

Tighten
Tighten the lower accelerator pedal retaining bolt to 23 N·m (17 lb ft).

3. Connect the ETC connector to the accelerator pedal.