For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the luggage compartment lock cover.
3. Disconnect the electrical connector.
4. Remove the screws and the luggage compartment lock.
5. Disconnect the lock rod.

### Installation Procedure

1. Connect the lock rod.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the luggage compartment lock with the screws.

Tighten
Tighten the luggage compartment lock screws to 8 N·m (71 lb in).

3. Connect the electrical connector.
4. Install the luggage compartment lock cover.
5. Connect the negative battery cable.