For 1990-2009 cars

### Removal Procedure

1. Remove the front molding (1) bonded by the two sided tape.
2. Remove the front lower fascia extension screws.
3. Remove the side lower screws from the front lower fascia extension.
4. Remove the side screws and the retaining clips from the front lower fascia extension.
5. Remove the nuts from the front lower fascia extension.
6. Remove the front lower fascia extension from the vehicle.

### Installation Procedure

1. Install the front lower fascia extension.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front lower fascia extension nuts and tighten to 2 N·m (18 lb in).
3. Install the side screws and the lower retaining clips. Tighten the side screws to 2 N·m (18 lb in).
4. Install the lower fascia extension lower screws and tighten to 2 N·m (18 lb in).
5. Install the lower fascia extension screws and tighten to 2 N·m (18 lb in).
6. Apply new 2-way tape and install the front lower fascia extension molding (1).