For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the intermediate drive shaft.

1 | Right Front Wheel Drive Shaft Oil Seal Tip

• | For seal removal use J 6125-B Slide Hammer with J 23129 Universal Seal Remover.

• | For seal installation use J 8092 Driver Handle with DT-47790 Seal Installer.

#### Special Tools

• | DT-47790 Seal Installer

• | J 6125-B Slide Hammer

• | J 8092 Driver Handle

• | J 23129 Universal Seal Remover