For 1990-2009 cars

### Chime Module

The chine module will sound to bring attention to 1 or more of the following conditions:

• | The lights are on and the ignition is not in ACC, ON, or START.

• | The ignition key is in the ignition switch when the driver's side door is open.

• | The seat belt is unbuckled when the ignition is in ACC, ON, or START.

Voltage is supplied at all times through the fuse block to power the chime module.

### Headlamps-On Reminder

When the headlamp switch is in the headlamps-on or parking lamps-on positions, voltage is applied to the chime module. With the headlamp switch on and the driver's side door open, the module loses voltage. The module senses this change. If voltage is still available, it is applied to sound the chime. The chime can be turned off by turning the headlamp switch off or closing the driver's side door. To replace the chime module, refer to Chime Inoperative .