For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the bolt and disconnect the hose from the clutch release cylinder.
3. Remove the clutch release cylinder bolts and remove the release cylinder from the transaxle.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Connect the release cylinder to the transaxle and install the bolts and tighten to 15 N·m (11 lb ft).
2. Connect the hose assembly to the cylinder body.
3. Apply grease where the pushrod connects to the release lever. Be careful not to stain the boot.
4. Bleed the air. Refer to Hydraulic Clutch Bleeding.
5. Fill the reservoir with clutch/brake fluid up to the MAX level.
6. Connect the negative battery cable.