For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Housing Assembly Retaining Bolts | 12 N·m | 106 lb in
Band Clamp Bolt | 5 N·m | 44 lb in
Clamp Bolts | 4 N·m | 35 lb in
Clutch Plate and Hub Assembly Retaining Nut | 17 N·m | 13 lb ft
Condenser Mount Nuts | 8.5 N·m | 75 lb in
Discharge Hose Connecting Block-to-Compressor Retaining Nut | 33 N·m | 24 lb ft
Discharge Hose Connecting Block-to-Condenser Retaining Nut | 16 N·m | 12 lb ft
Expansion Valve Bolts | 10 N·m | 89 lb in
Front Compressor-to-Bracket Mounting Bolts | 27 N·m | 20 lb ft
High-Pressure Pipe-to-Evaporator Flange Connecting Block Nut | 10 N·m | 89 lb in
High-Pressure Pipe-to-Receiver-Dryer Connecting Block Nut | 10 N·m | 89 lb in
Liquid Condenser Pipe Nut | 15 N·m | 15 lb ft
Liquid Evaporator Pipe Clamp Bolt | 5 N·m | 44 lb in
Pressure Relief Valve | 16 N·m | 12 lb ft
Pressure Transducer | 7 N·m | 62 lb in
Rear Compressor-to-Bracket Mounting Bolts | 20 N·m | 15 lb ft
Receiver-Dryer to Condenser Pipe Nut | 14 N·m | 10 lb ft
Suction Hose Clamp Bolt | 10 N·m | 89 lb in
Suction Hose Connecting Block Retaining Nuts | 10 N·m | 89 lb in
Suction Hose Support Clamp Retaining Bolt | 5 N·m | 44 lb in
Suction Hose Support Clamp Retaining Nut | 5 N·m | 44 lb in
Through-Bolts | 10 N·m | 89 lb in
Vacuum Tank-to-Fire Wall Nuts | 4 N·m | 35 lb in