For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the console. Refer to Front Floor Console Replacement.
3. Disconnect the shift control cables from the shift control lever housing. Refer to Shift Control Linkage Replacement.
4. Remove the nuts and bolts from the shift control lever housing.
5. Remove the shift control lever housing.

### Installation Procedure

1. Install the shift control lever housing.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts and bolts to the shift control lever housing and tighten to 8 N·m (71 lb in).
3. Connect the shift control cables to the shift control lever housing, and adjust the cable. Refer to Shift Control Linkage Replacement.
4. Install the console. Refer to Front Floor Console Replacement.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.