For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Detent Spring Retaining Bolt (16.7 mm) | 10 N·m | 89 lb in
Detent Spring Retaining Bolt (14 mm) | 6 N·m | 53 lb in
Differential Gear Lube Apply Tube Clamp Bolt | 6 N·m | 53 lb in
Drain Plug | 40 N·m | 30 lb ft
Flywheel-to-Torque Converter Bolts | 45 N·m | 33 lb ft
Forward Clutch (C1) Accumulator Bolt | 10 N·m | 89 lb in
Front Damper Bush Bracket Bolts | 65 N·m | 48 lb ft
Inlet Pipe Union Bolt | 33 N·m | 24 lb ft
Input Speed Sensor Bolt | 6 N·m | 53 lb in
Left 3 Transaxle Mounting Bracket Bolts | 40 N·m | 30 lb ft
Left Lower Engine-to-Transaxle Bolts | 73 N·m | 54 lb ft
Oil Apply Tube Clamp Retaining Bolt | 6 N·m | 53 lb in
Oil Cooler Line Assembly Bolt | 10 N·m | 89 lb in
Oil Level Gage Bolt | 10 N·m | 89 lb in
Oil Pan Flange-to-Transaxle Bolts | 31 N·m | 23 lb ft
Oil Pump Assembly Bolt | 25 N·m | 18 lb ft
Oil Pump Cover Bolt (14 mm) | 12 N·m | 106 lb in
Oil Pump Cover Bolt (17 mm) | 7 N·m | 62 lb in
Oil Reservoir Plate (Transaxle Case) Bolt | 6 N·m | 53 lb in
Oil Reservoir Plate (Transaxle Housing) Bolt | 8 N·m | 53 lb in
Oil Strainer Bolt | 6 N·m | 53 lb in
Outlet Pipe Clip Bolt | 9 N·m | 80 lb in
Outlet Pipe Union Bolt | 33 N·m | 24 lb ft
Output Speed Sensor Bolt | 6 N·m | 53 lb in
Rear Case Bolt | 30 N·m | 22 lb ft
Rear Transaxle Mounting Bracket Bolt | 65 N·m | 48 lb ft
Right Lower Engine-to-Transaxle Bolts | 73 N·m | 54 lb ft
Shift Control Knob Bolts | 2 N·m | 18 lb in
Shift Control Lever Assembly Mounting Bolts | 8 N·m | 71 lb in
Side Cover Bolt | 13 N·m | 10 lb in
Solenoid Bolt | 7 N·m | 62 lb in
Suction Cover Bolt | 10 N·m | 89 lb in
TCM Retaining Nuts | 15 N·m | 11 lb ft
TFT Sensor Bolt | 10 N·m | 89 lb in
Transaxle Case Plate Bolt | 6 N·m | 53 lb in
Transaxle Housing Bolt | 30 N·m | 22 lb ft
Transaxle Mounting Bracket Cage Bolt and Nut | 65 N·m | 48 lb ft
Transmission Range (TR) Switch Bolts | 25 N·m | 18 lb ft
Transmission Range (TR) Lever Nut | 16 N·m | 12 lb ft
Transmission Range (TR) Switch Nut | 7 N·m | 62 lb in
Torsion Spring Retaining Bolt No. 2 | 10 N·m | 89 lb in
Underdrive Brake (B4) Anchor Bolt | 167 N·m | 123 lb ft
Underdrive Brake (B4) Apply Tube Clamp Retaining Bolt | 6 N·m | 53 lb in
Underdrive Clutch Bolt | 7 N·m | 62 lb in
Upper Transaxle-to-Engine Bolts | 73 N·m | 54 lb ft
Valve Body Assembly Bolt | 10 N·m | 89 lb in