For 1990-2009 cars

### Removal Procedure

1. Remove the bolt securing the lock cylinder.
2. Disconnect the lock rod.
3. Disconnect the electrical connector.
4. Remove the luggage compartment lock cylinder.

### Installation Procedure

1. Install the luggage compartment lock cylinder.
2. Connect the electrical connector.
3. Connect the lock rod.

Caution: Refer to Fastener Caution in the Preface section.

4. Secure the luggage compartment lock cylinder with the bolt and tighten to 8 N·m (71 lb in).