For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Camshaft Position (CMP) Sensor Retaining Bolt | 12 N·m | 106 lb in
Crankshaft Position (CKP) Sensor Heat Shield Housing Bolt | 8 N·m | 71 lb in
Crankshaft Position (CKP) Sensor Retaining Bolt | 7 N·m | 62 lb in
Engine Control Module (ECM) Bracket Nut | 12 N·m | 106 lb in
Engine Control Module (ECM) Retaining Nut | 12 N·m | 106 lb in
Engine Coolant Temperature (ECT) Sensor | 17 N·m | 13 lb ft
Exhaust Gas Recirculation (EGR) Adapter Retaining Bolt | 20 N·m | 15 lb ft
Exhaust Gas Recirculation (EGR) Pipe Retaining Bolt/Nut | 10 N·m | 89 lb in
Exhaust Gas Recirculation (EGR) Pipe-to-Bracket Cylinder Head Long Side Retaining Bolt | 10 N·m | 89 lb in
Exhaust Gas Recirculation (EGR) Pipe-to-Bracket Cylinder Head Short Side Retaining Bolt | 20 N·m | 15 lb ft
Exhaust Gas Recirculation (EGR) Valve Retaining Bolt | 25 N·m | 18 lb ft
Fuel Filter Protector Retaining Bolt | 4 N·m | 35 lb in
Fuel Pressure Regulator Retaining Bolt | 12 N·m | 106 lb in
Ignition Coil Retaining Bolt | 7 N·m | 62 lb in
Intake Air Temperature (IAT) Sensor | 25 N·m | 18 lb ft
Intake Exhaust Gas Recirculation (EGR) Pipe Retaining Bolt | 10 N·m | 89 lb in
Knock Sensor Retaining Bolt | 19 N·m | 14 lb ft
Manifold Absolute Pressure (MAP) Sensor | 8 N·m | 71 lb in
Oxygen Sensor (O2S) | 39 N·m | 29 lb ft
Spark Plug | 25 N·m | 18 lb ft
Throttle Body Assembly Retaining Bolt | 13 N·m | 115 lb in
Variable Intake System (VIS) Actuator Retaining Bolt | 12 N·m | 106 lb in
Variable Intake System (VIS) Vacuum Tank Retaining Bolt | 8 N·m | 71 lb in
Variable Intake System (VIS) Valve Retaining Bolt | 12 N·m | 106 lb in