For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat back.
2. Remove the rear seat side bolster cushion. Refer to Seat Back Cushion Side Bolster Panel Replacement.
3. Remove the retaining clips and the back panel trim cover.
4. Remove the bolts and the seat back lock strikers.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat back lock strikers with the bolts and tighten to 25 N·m (18 lb ft).
2. Install the back panel trim cover with the retaining clips.
3. Install the rear seat side bolster cushion. Refer to Seat Back Cushion Side Bolster Panel Replacement.
4. Raise and secure the rear seat backs in the upright position.