For 1990-2009 cars

### Removal Procedure

1. Remove the screws and the sun visor from the headliner.
2. Disconnect the vanity mirror electrical connector. Refer to Vanity Mirror Lamp Replacement.
3. Remove the screw and the sun visor support from the headliner.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the sun visor support to the headliner with the screw and tighten to 1.5 N·m (13 lb in).
2. Connect the vanity mirror electrical connector. Refer to Vanity Mirror Lamp Replacement.
3. Install the sun visor to the headliner with the screws and tighten to 4 N·m (35 lb in)..