For 1990-2009 cars

### Removal Procedure

1. Remove the control valve body assembly. Refer to Control Valve Body Replacement.
2. Remove the input speed sensor bolt.
3. Remove the sensor and seals.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the input speed sensor, the bolt, and seals (1).

Tighten
Tighten the input speed sensor bolt to 12 N·m (106 lb in).

2. Install the control valve body assembly. Refer to Control Valve Body Replacement.