For 1990-2009 cars

### Removal Procedure

1. Remove the rear molding (1) bonded by the 2-sided tape.
2. Remove the upper screws.
3. Remove the rear side screws.
4. Remove the retaining clips and the lower screws.
5. Remove the nuts.
6. Remove the rear lower fascia extension.

### Installation Procedure

1. Install the lower fascia extension.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts and tighten to 2 N·m (18 lb in).
3. Install the lower screws and clips and tighten to 2 N·m (18 lb in).
4. Install the side screws and tighten to 2 N·m (18 lb in).
5. Install the center screws and tighten to 2 N·m (18 lb in).
6. Install new 2-sided tape to the rear molding and install the rear molding (1) to the rear lower fascia extension.