For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transaxle brace bolts (1, 3).
3. Remove the transaxle brace (2).

### Installation Procedure

1. Install the transaxle brace (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transaxle brace bolt (1) and tighten to 50 N·m (37 lb ft).
3. Install the transaxle brace bolt (3) and tighten to 100 N·m (74 lb ft).
4. Lower the vehicle.