For 1990-2009 cars

## Fastener Tightening Specifications Gasoline Engine

Application | Specification
--- | ---
Metric | English
Battery Cable Nuts | 15 N·m | 11 lb ft
Battery Carrier Tray Lower Bolts | 10 N·m | 89 lb in
Battery Carrier Tray Upper Bolts | 20 N·m | 15 lb ft
Battery Retainer Clamp-to-Battery Rod Nuts | 4N·m | 35 lb in
Battery Terminal Bolts | 20 N·m | 15 lb ft
Battery-to-Generator Lead Nut | 15 N·m | 11 lb ft
Generator Driveshaft Nut | 100 N·m | 74 lb ft
Generator Lower Bracket-to-Engine Block Bolts | 35 N·m | 26 lb ft
Generator Lower Bracket-to-Generator Nut | 35 N·m | 26 lb ft
Generator Through-Bolts | 25 N·m | 18 lb ft
Generator-to-Cylinder Head Support Bracket Bolt | 20 N·m | 15 lb ft
Generator-to-Intake Manifold and Cylinder Head Support Bracket Bolts | 35 N·m | 26 lb ft
Generator-to-Intake Manifold Strap Bracket Bolt | 20 N·m | 15 lb ft
Intake Manifold-to-Engine Block Bracket Bolts (Over Starter) | 20 N·m | 15 lb ft
Starter Field Connector Nut | 8 N·m | 71 lb in
Starter Solenoid Assembly Screws | 8 N·m | 71 lb in
Starter Solenoid Terminal-to-Battery Cable Terminal Nut | 15 N·m | 11 lb ft
Starter Solenoid Terminal-to-Ignition Solenoid Terminal Nut | 6 N·m | 53 lb in
Starter Through-Bolts | 6 N·m | 53 lb in
Starter-to-Engine Block Mounting Bolt | 45 N·m | 33 lb ft
Starter-to-Transmission Mounting Bolt | 50 N·m | 37 lb in

## Fastener Tightening Specifications Diesel Engine

Application | Specification
--- | ---
Metric | English
Battery Ground Retaining Nut | 10 N·m | 89 lb in
Battery Hold-Down Bar Bracket Retaining Nut | 4 N·m | 35 lb in
Battery Terminal Nut | 4.5 N·m | 40 lb in
Battery Tray Bolts | 20 N·m | 15 lb ft
Generator B+ Wiring Harness Retaining Nut | 25 N·m | 18 lb ft
Generator Bolt | 30 N·m | 22 lb ft
Generator Drive And Bearing Nut | 81 N·m | 60 lb ft
Generator Through-Bolt | 10 N·m | 89 lb in
Glow Plug Fuse Box Retaining Bolt | 10 N·m | 89 lb in
Starter Solenoid Terminal-to-Battery Lead Wire Nut | 15 N·m | 11 lb ft
Starter Field Coil Connector Nut | 8 N·m | 71 lb in
Starter Solenoid Assembly Screw | 8 N·m | 71 lb in
Starter-to-Engine Block Mounting Bolt | 45 N·m | 33 lb ft
Starter Through-Bolt | 6 N·m | 53 lb in