For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connectors.
3. Remove the nuts and the lamp assembly.
4. Remove any inoperative bulb.

### Installation Procedure

1. Install the replacement bulbs.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the lamp assembly with the nuts.

Tighten
Tighten the rear combination lamp assembly nuts to 2 N·m (18 lb in).

3. Connect the electrical connectors.
4. Connect the negative battery cable.