For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
021 |  | BCM | DTC 021
022 | Front Washer Request Signal Circuit | BCM | DTC 022
023 | Keyless Entry Transmitter Low Battery | TDM | DTC 023
024 | Keyless Entry Transmitter Synchronization Failure | TDM | DTC 024
025 |  | BCM | DTC 025-026
026 |  | BCM | DTC 025-026
027 |  | BCM | DTC 027-028
028 |  | BCM | DTC 027-028
029 |  | BCM | DTC 029
033 | Immobilizer Antenna Incorrect Value | TDM | DTC 033
034 | Absence of Immobilizer Antennae/Link Error | TDM | DTC 034
035 | Link Immobilizer Antenna Error | TDM | DTC 035
B1101 | Battery Voltage High | SDM | DTC B1101
B1102 | Battery Voltage Low | SDM | DTC B1102
B1103 | SIR Serial Communications Fault | SDM | DTC B1103
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379
B1380 | LF Side Deployment Loop Shorted to Ground | SDM | DTC B1380
B1381 | LF Side Deployment Loop Shorted to Battery | SDM | DTC B1381
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383
B1384 | RF Side Deployment Loop Shorted to Ground | SDM | DTC B1384
B1385 | RF Side Deployment Loop Shorted to Battery | SDM | DTC B1385
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395
B1400 | Driver SIS Malfunction | SDM | DTC B1400
B1401 | LF Side Impact Sensor (SIS) Short to Ground | SDM | DTC B1401
B1402 | LF Side Impact Sensor (SIS) Short to Battery | SDM | DTC B1402
B1403 | Passenger SIS Malfunction | SDM | DTC B1403
B1404 | RF Side Impact Sensor (SIS) Short to Ground | SDM | DTC B1404
B1405 | RF Side Impact Sensor (SIS) Short to Battery | SDM | DTC B1405
B1406 | PPD/SBR Malfunction | SDM | DTC B1406
B1407 | PPD/SBR Communication Error | SDM | DTC B1407
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415
B1453 | Vehicle Speed Signal | SDM | DTC B1453
B1473 | Left Roof Rail Deployment Loop Resistance Above Threshold | SDM | DTC B1473
B1474 | Left Roof Rail Deployment Loop Resistance Low | SDM | DTC B1474
B1475 | LH Roof Rail Deployment Loop Short to Ground | SDM | DTC B1475
B1476 | Left Roof Rail Deployment Loop Short to Battery | SDM | DTC B1476
B1477 | Right Roof Rail Deployment Loop Resistance Above Threshold | SDM | DTC B1477
B1478 | Right Roof Rail Deployment Loop Resistance Low | SDM | DTC B1478
B1479 | RH Roof Rail Deployment Loop Short to Ground | SDM | DTC B1479
B1480 | Right Roof Rail Deployment Loop Short to Battery | SDM | DTC B1480
B1620 | Electronic Control Unit Performance | SDM | DTC B1620
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502
C0730 | CAN Gear Signal Error | EBCM/ESC/TCS | DTC C0730
C1101 | Battery Voltage High | EBCM | DTC C1101
C1102 | Battery Voltage Low | EBCM | DTC C1102
C1200 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1200
C1201 | Left Front Wheel Speed Circuit Range Performance | EBCM | DTC C1201
C1202 | Left Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1202
C1203 | Right Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1203
C1204 | Right Front Wheel Speed Circuit Range Performance | EBCM | DTC C1204
C1205 | Right Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1205
C1206 | Left Rear Wheel Speed Sensor Circuit Shorted or Open | EBCM | DTC C1206
C1207 | Left Rear Wheel Speed Sensor Circuit Range Performance | EBCM | DTC C1207
C1208 | Left Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1208
C1209 | Right Rear Wheel Speed Circuit Shorted or Open | EBCM | DTC C1209
C1210 | Right Rear Wheel Speed Circuit Range Performance | EBCM | DTC C1210
C1211 | Right Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1211
C1503 | Traction Control Switch Circuit | EBCM | DTC C1503
C1604 | ECU Malfunction | EBCM | DTC C1604
C1605 | CAN Bus Error | EBCM | DTC C1605, C1611, C1612, or C1616
C1611 | CAN Bus Error | EBCM | DTC C1605, C1611, C1612, or C1616
C1612 | CAN Bus Error | EBCM | DTC C1605, C1611, C1612, or C1616
C1616 | CAN Bus OFF Failure | EBCM | DTC C1605, C1611, C1612, or C1616
C2112 | Solenoid Valve Relay Circuit | EBCM | DTC C2112 or C2380
C2380 | Solenoid Valve Circuit | EBCM | DTC C2112 or C2380
C2402 | Pump Motor Circuit | EBCM | DTC C2402
P0016 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0016 or P0340 for the 2.0L and 2.5L engine
P0016 5A | Camshaft Position (CMP) Sensor Circuit Plausibility Failure | ECM | DTC P0016, P0340, or P0341 for the 2.0L diesel engine
P0030 | H02S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0031 | H02S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0032 | H02S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0036 | H02S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0037 | H02S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0038 | H02S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0045 01 | Turbocharge Boost Control Solenoid Control Circuit Short to Battery | ECM | DTC P0045, P0047, or P0048 for the 2.0L diesel engine
P0045 02 | Turbocharge Boost Control Solenoid Control Circuit Short to Ground | ECM | DTC P0045, P0047, or P0048 for the 2.0L diesel engine
P0045 04 | Turbocharge Boost Control Solenoid Control Circuit Open | ECM | DTC P0045, P0047, or P0048 for the 2.0L diesel engine
P0045 54 | Turbocharge Boost Control Solenoid Control Circuit Temperature High | ECM | DTC P0045, P0047, or P0048 for the 2.0L diesel engine
P0047 | Turbocharge Boost Control Solenoid Control Circuit Low Voltage | ECM | DTC P0045, P0047, or P0048 for the 2.0L diesel engine
P0048 | Turbocharge Boost Control Solenoid Control Circuit High Voltage | ECM | DTC P0045, P0047, or P0048 for the 2.0L diesel engine
P0050 | H02S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0051 | H02S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0052 | H02S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0056 | H02S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0057 | H02S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0058 | H02S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0069 | Manifold Absolute Pressure Barometric Pressure Correlation | ECM | DTC P0069 for the 2.0L diesel engine
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0089 for the 2.0L diesel engine
P0089 11 | Fuel Pressure Regulator Performance Above Maximum Threshold | ECM | DTC P0089 for the 2.0L diesel engine
P0089 12 | Fuel Pressure Regulator Performance Below Minimum Threshold | ECM | DTC P0089 for the 2.0L diesel engine
P0089 18 | Fuel Pressure Regulator Performance Signal Amplitude Less Than Minimum | ECM | DTC P0089 for the 2.0L diesel engine
P0089 19 | Fuel Pressure Regulator Performance Signal Amplitude Greater Than Maximum | ECM | DTC P0089 for the 2.0L diesel engine
P0090 01 | Fuel Pressure Regulator Solenoid 1 Control Circuit Short to Battery | ECM | DTC P0090, P0091, or P0092 for the 2.0L diesel engine
P0090 02 | Fuel Pressure Regulator Solenoid 1 Control Circuit Short to Ground | ECM | DTC P0090, P0091, or P0092 for the 2.0L diesel engine
P0090 04 | Fuel Pressure Regulator Solenoid 1 Control Circuit Open | ECM | DTC P0090, P0091, or P0092 for the 2.0L diesel engine
P0091 | Fuel Pressure Regulator Solenoid 1 Control Circuit Low Voltage | ECM | DTC P0090, P0091, or P0092 for the 2.0L diesel engine
P0092 | Fuel Pressure Regulator Solenoid 1 Control Circuit High Voltage | ECM | DTC P0090, P0091, or P0092 for the 2.0L diesel engine
P0095 03 | Intake Air Temperature (IAT) Sensor 2 Circuit Voltage Below Threshold | ECM | DTC P0095, P0097, or P0098 for the 2.0L diesel engine
P0095 07 | Intake Air Temperature (IAT) Sensor 2 Circuit Voltage Above Threshold | ECM | DTC P0095, P0097, or P0098 for the 2.0L diesel engine
P0097 | Intake Air Temperature (IAT) Sensor 2 Circuit Low Voltage | ECM | DTC P0095, P0097, or P0098 for the 2.0L diesel engine
P0098 | Intake Air Temperature (IAT) Sensor 2 Circuit High Voltage | ECM | DTC P0095, P0097, or P0098 for the 2.0L diesel engine
P0100 | Mass Air Flow (MAF) Sensor Circuit Signal | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0100 09 | Mass Air Flow (MAF) Sensor Circuit Rate of Change Above Threshold | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0100 0A | Mass Air Flow (MAF) Sensor Circuit Rate of Change Below Threshold | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0100 26 | Mass Air Flow (MAF) Sensor Circuit Frequency Too Low | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0100 27 | Mass Air Flow (MAF) Sensor Circuit Frequency Too High | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101, P0102, or P0103 for the 2.0L and 2.5L engine
P0101 11 | Mass Air Flow (MAF) Sensor Performance Above Maximum | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0102 | Mass Air Flow (MAF) Low Frequency | ECM | DTC P0101, P0102, or P0103 for the 2.0L and 2.5L engine or DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0103 | Mass Air Flow (MAF) High Frequency | ECM | DTC P0101, P0102, or P0103 for the 2.0L and 2.5L engine or DTC P0100, P0101, P0102, or P0103 for the 2.0L diesel engine
P0105 03 | Manifold Absolute Pressure (MAP) Sensor Circuit Voltage Below Threshold | ECM | DTC P0105, P0107, or P0108 for the 2.0L diesel engine
P0105 07 | Manifold Absolute Pressure (MAP) Sensor Circuit Voltage Above Threshold | ECM | DTC P0105, P0107, or P0108 for the 2.0L diesel engine
P0105 5A | Manifold Absolute Pressure (MAP) Sensor Circuit Plausibility Failure | ECM | DTC P0105, P0107, or P0108 for the 2.0L diesel engine
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM | DTC P0107 or P0108 for the 2.0L and 2.5L engine or DTC P0105, P0107, or P0108 for the 2.0L diesel engine
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM | DTC P0107 or P0108 for the 2.0L and 2.5L engine or DTC P0105, P0107, or P0108 for the 2.0L diesel engine
P0110 | Intake Air Temperature (IAT) Sensor 1 Circuit | ECM | DTC P0110 for the 2.0L diesel engine
P0110 09 | Intake Air Temperature (IAT) Sensor 1 Circuit Rate of Change Above Threshold | ECM | DTC P0110 for the 2.0L diesel engine
P0110 0A | Intake Air Temperature (IAT) Sensor 1 Circuit Rate of Change Below Threshold | ECM | DTC P0110 for the 2.0L diesel engine
P0110 11 | Intake Air Temperature (IAT) Sensor 1 Circuit Above Maximum Threshold | ECM | DTC P0110 for the 2.0L diesel engine
P0110 12 | Intake Air Temperature (IAT) Sensor 1 Circuit Below Minimum Threshold | ECM | DTC P0110 for the 2.0L diesel engine
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112 or P0113 for the 2.0L and 2.5L engine
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112 or P0113 for the 2.0L and 2.5L engine
P0115 03 | Engine Coolant Temperature (ECT) Sensor Circuit Voltage Below Threshold | ECM | DTC P0115, P0116, P0117, or P0118 for the 2.0L diesel engine
P0115 07 | Engine Coolant Temperature (ECT) Sensor Circuit Voltage Above Threshold | ECM | DTC P0115, P0116, P0117, or P0118 for the 2.0L diesel engine
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0115, P0116, P0117, or P0118 for the 2.0L diesel engine
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 or P0118 for the 2.0L and 2.5L engine or DTC P0115, P0116, P0117, or P0118 for the 2.0L diesel engine
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117 or P0118 for the 2.0L and 2.5L engine or DTC P0115, P0116, P0117, or P0118 for the 2.0L diesel engine
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.0L and 2.5L engine
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.0L and 2.5L engine
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.0L and 2.5L engine
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.0L and 2.5L engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.0L and 2.5L engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.0L and 2.5L engine
P0131 | H02S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131 or P0151 for the 2.0L and 2.5L engine
P0132 | H02S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0132 or P0152 for the 2.0L and 2.5L engine
P0133 | H02S/02S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 or P0153 for the 2.0L and 2.5L engine
P0134 | H02S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0134 or P0154 for the 2.0L and 2.5L engine
P0135 | H02S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.0L and 2.5L engine
P0137 | H02S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0137 or P0157 for the 2.0L and 2.5L engine
P0138 | H02S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0138 or P0158 for the 2.0L and 2.5L engine
P0139 | H02S Slow Response Bank 1 Sensor 2 | ECM | DTC P0139 or P0159 for the 2.0L and 2.5L engine
P0140 | H02S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0140 or P0160 for the 2.0L and 2.5L engine
P0141 | H02S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.0L and 2.5L engine
P0151 | H02S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151 for the 2.0L and 2.5L engine
P0152 | H02S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152 for the 2.0L and 2.5L engine
P0153 | H02S/02S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153 for the 2.0L and 2.5L engine
P0154 | H02S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0134 or P0154 for the 2.0L and 2.5L engine
P0155 | H02S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.0L and 2.5L engine
P0157 | H02S Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137 or P0157 for the 2.0L and 2.5L engine
P0158 | H02S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0138 or P0158 for the 2.0L and 2.5L engine
P0159 | H02S Slow Response Bank 2 Sensor 2 | ECM | DTC P0139 or P0159 for the 2.0L and 2.5L engine
P0160 | H02S Circuit Insufficient Activity Bank 2 Sensor 2 | ECM | DTC P0140 or P0160 for the 2.0L and 2.5L engine
P0161 | H02S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.0L and 2.5L engine
P0171 | Fuel Trim System Lean Bank 1 | ECM | DTC P0171, P0172, P0174, or P0175 for the 2.0L and 2.5L engine
P0172 | Fuel Trim System Rich Bank 1 | ECM | DTC P0171, P0172, P0174, or P0175 for the 2.0L and 2.5L engine
P0174 | Fuel Trim System Lean Bank 2 | ECM | DTC P0171, P0172, P0174, or P0175 for the 2.0L and 2.5L engine
P0175 | Fuel Trim System Rich Bank 2 | ECM | DTC P0171, P0172, P0174, or P0175 for the 2.0L and 2.5L engine
P0180 03 | Fuel Temperature Sensor Circuit Voltage Below Threshold | ECM | DTC P0180, P0182, or P0183 for the 2.0L diesel engine
P0180 07 | Fuel Temperature Sensor Circuit Voltage Above Threshold | ECM | DTC P0180, P0182, or P0183 for the 2.0L diesel engine
P0182 | Fuel Temperature Sensor Circuit Low Voltage | ECM | DTC P0180, P0182, or P0183 for the 2.0L diesel engine
P0183 | Fuel Temperature Sensor Circuit High Voltage | ECM | DTC P0180, P0182, or P0183 for the 2.0L diesel engine
P0190 03 | Fuel Rail Pressure (FRP) Sensor Circuit Voltage Below Threshold | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0190 07 | Fuel Rail Pressure (FRP) Sensor Circuit Voltage Above Threshold | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0190 11 | Fuel Rail Pressure (FRP) Sensor Circuit Voltage Above Maximum Threshold | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0190 12 | Fuel Rail Pressure (FRP) Sensor Circuit Voltage Below Minimum Threshold | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0191 | Fuel Rail Pressure (FRP) Sensor Performance | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0192 | Fuel Rail Pressure (FRP) Sensor Circuit Low Voltage | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0193 | Fuel Rail Pressure (FRP) Sensor Circuit High Voltage | ECM | DTC P0190, P0191, P0192, or P0193 for the 2.0L diesel engine
P0201 | Fuel Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0201 04 | Fuel Injector 1 Control Circuit Open | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0 diesel engine
P0202 | Fuel Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0202 04 | Fuel Injector 2 Control Circuit Open | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0203 | Fuel Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0203 04 | Fuel Injector 3 Control Circuit Open | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0204 | Fuel Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0204 04 | Fuel Injector 4 Control Circuit Open | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0222 | Throttle Position (TP) Sensor 2 Low Voltage | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0223 | Throttle Position (TP) Sensor 2 High Voltage | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.0L and 2.5L engine
P0230 | Fuel Pump Relay Control Circuit | ECM | DTC P0230 for the 2.0L and 2.5L engine
P0234 | Turbocharge Engine Overboost | ECM | DTC P0234 or P0299 for the 2.0L diesel engine
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0263 11 | Cylinder 1 Balance System Above Maximum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0263 12 | Cylinder 1 Balance System Below Minimum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0266 11 | Cylinder 2 Balance System Above Maximum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0266 12 | Cylinder 2 Balance System Below Minimum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0269 11 | Cylinder 3 Balance System Above Maximum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0269 12 | Cylinder 3 Balance System Below Minimum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0272 11 | Cylinder 4 Balance System Above Maximum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0272 12 | Cylinder 4 Balance System Below Minimum Threshold | ECM | DTC P0263, P0266, P0269, or P0272 for the 2.0L diesel engine
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.0L and 2.5L engine
P0299 | Turbocharge Engine Underboost | ECM | DTC P0234 or P0299 for the 2.0L diesel engine
P02E0 | Intake Air (IA) Flow Valve Control Circuit | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P02E0 01 | Intake Air (IA) Flow Valve Control Circuit Short to Battery | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P02E0 02 | Intake Air (IA) Flow Valve Control Circuit Short to Ground | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P02E0 04 | Intake Air (IA) Flow Valve Control Circuit Open Circuit | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P02E0 54 | Intake Air (IA) Flow Valve Control Circuit Open Circuit High Temperature | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P02E1 11 | Intake Air (IA) Flow Valve Control Performance Above Maximum Threshold | ECM | DTC P02E1 for the 2.0L diesel engine
P02E1 12 | Intake Air (IA) Flow Valve Control Performance Below Minimum Threshold | ECM | DTC P02E1 for the 2.0L diesel engine
P02E2 | Intake Air (IA) Flow Valve Control Circuit Low Voltage | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P02E3 | Intake Air (IA) Flow Valve Control Circuit High Voltage | ECM | DTC P02E0, P02E2, or P02E3 for the 2.0L diesel engine
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0306 for the 2.0L and 2.5L engine
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0306 for the 2.0 L and 2.5 L engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0306 for the 2.0L and 2.5L engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0306 for the 2.0L and 2.5L engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0306 for the 2.0L and 2.5L engine
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306 for the 2.0L and 2.5L engine
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306 for the 2.0L and 2.5L engine
P0325 | Knock Sensor (KS) 1 Circuit | ECM | DTC P0325, P0326, P0330, or P0331 for the 2.0L and 2.5L engine
P0326 | Knock Sensor (KS) 1 Performance | ECM | DTC P0325, P0326, P0330, or P0331 for the 2.0L and 2.5L engine
P0330 | Knock Sensor (KS) 2 Circuit | ECM | DTC P0325, P0326, P0330, or P0331 for the 2.0L and 2.5L engine
P0331 | Knock Sensor (KS) 2 Performance | ECM | DTC P0325, P0326, P0330, or P0331 for the 2.0L and 2.5L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335 or P0336 for the 2.0L and 2.5L engine or DTC P0335 or P0336 for the 2.0L diesel engine
P0335 28 | Crankshaft Position (CKP) Sensor Circuit Incorrect Frequency | ECM | DTC P0335 or P0336 for the 2.0L diesel engine
P0335 29 | Crankshaft Position (CKP) Sensor Circuit Too Few Pulses | ECM | DTC P0335 or P0336 for the 2.0L diesel engine
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335 or P0336 for the 2.0L and 2.5L engine
P0336 | Crankshaft Position (CKP) Sensor Circuit Performance | ECM | DTC P0335 or P0336 for the 2.0L diesel engine
P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016 or P0340 for the 2.0L and 2.5L engine
P0340 28 | Camshaft Position (CMP) Sensor Circuit Incorrect Frequency | ECM | DTC P0016, P0340, or P0341 for the 2.0L diesel engine
P0340 29 | Camshaft Position (CMP) Sensor Circuit Too Few Pulses | ECM | DTC P0016, P0340, or P0341 for the 2.0L diesel engine
P0341 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016, P0340, or P0341 for the 2.0L diesel engine
P0381 | Wait to Start Lamp Control Circuit | ECM | DTC P0381 for the 2.0L diesel engine
P0381 01 | Wait to Start Lamp Control Circuit Short to Battery | ECM | DTC P0381 for the 2.0L diesel engine
P0381 02 | Wait to Start Lamp Control Circuit Short to Ground | ECM | DTC P0381 for the 2.0L diesel engine
P0381 04 | Wait to Start Lamp Control Circuit Open Circuit | ECM | DTC P0381 for the 2.0L diesel engine
P0381 54 | Wait to Start Lamp Control Circuit Temperature High | ECM | DTC P0381 for the 2.0L diesel engine
P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM | DTC P0400, P0401, or P0402 for the 2.0L and 2.5L engine
P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM | DTC P0400, P0401, or P0402 for the 2.0L and 2.5L engine or DTC P0401 or P0402 for the 2.0L diesel engine
P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM | DTC P0400, P0401, or P0402 for the 2.0L and 2.5L engine or DTC P0401 or P0402 for the 2.0L diesel engine
P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 2.0L and 2.5L engine or DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0403 01 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Short to Battery | ECM | DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0403 02 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Short to Ground | ECM | DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0403 04 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Open | ECM | DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0403 54 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Temperature High | ECM | DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 2.0L and 2.5L engine
P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 2.0L and 2.5L engine
P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 2.0L and 2.5L engine
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 or P0430 for the 2.0L and 2.5L engine
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430 for the 2.0L and 2.5L engine
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0458, or P0459 for the 2.0L and 2.5L engine
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.0L and 2.5L engine
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.0L and 2.5L engine
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480 or P0481
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480 or P0481
P0489 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Low Voltage | ECM | DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0490 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit High Voltage | ECM | DTC P0403, P0489, or P0490 for the 2.0L diesel engine
P0500 | Vehicle Speed Sensor (VSS) Circuit | ECM | DTC P0500 for the 2.0L and 2.5L engine or DTC P0500, P0502, or P0503 for the 2.0L diesel engine
P0500 08 | Vehicle Speed Sensor (VSS) Circuit Signal Invalid | ECM | DTC P0500, P0502, or P0503 for the 2.0L diesel engine
P0500 11 | Vehicle Speed Sensor (VSS) Circuit Above Maximum Threshold | ECM | DTC P0500, P0502, or P0503 for the 2.0L diesel engine
P0500 71 | Vehicle Speed Sensor (VSS) Circuit Invalid Serial Data Received | ECM | DTC P0500, P0502, or P0503 for the 2.0L diesel engine
P0502 | Vehicle Speed Sensor (VSS) Circuit Low Frequency | ECM | DTC P0500, P0502, or P0503 for the 2.0L diesel engine
P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM | DTC P0500, P0502, or P0503 for the 2.0L diesel engine
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 for the automatic HVAC or DTC P0532 or P0533 for the manual HVAC
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0533 for the automatic HVAC or DTC P0532 or P0533 for the manual HVAC
P0544 03 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit Voltage Below Threshold | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P0544 07 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit Voltage Above Threshold | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P0545 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit Low Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P0546 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit High Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P0564 | Cruise Control Multi-Function Switch Circuit | ECM | DTC P0564
P0602 46 | Control Module Not Programmed Vehicle Configuration Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L and 2.5L engine
P0605 | Control Module Programming Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L and 2.5L engine
P0606 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 3C | Control Module Internal Performance Internal Communication Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 11 | Control Module Internal Performance Above Maximum Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 12 | Control Module Internal Performance Below Minimum Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 31 | Control Module Internal Performance General Checksum Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 33 | Control Module Internal Performance Special Memory Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 37 | Control Module Internal Performance Watchdog/Safety Processor Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 5A | Control Module Internal Performance Plausibility Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0606 59 | Control Module Internal Performance Circuit/Component Protection Time Out | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0607 39 | Control Module Internal Electronic Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060A | Control Module Monitoring Processor Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060A 07 | Control Module Monitoring Processor Performance Voltage Above Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060B | Control Module Analog to Digital Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060B 03 | Control Module Analog to Digital Performance Voltage Below Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060B 07 | Control Module Analog to Digital Performance Voltage Above Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060B 08 | Control Module Analog to Digital Performance Signal Invalid | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P060B 11 | Control Module Analog to Digital Performance Above Maximum Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P061C | Control Module Engine Speed Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0627 01 | Fuel Pump Relay Control Circuit Short to Battery | ECM | DTC P0627 for the 2.0L diesel engine
P0627 02 | Fuel Pump Relay Control Circuit Short to Ground | ECM | DTC P0627 for the 2.0L diesel engine
P0627 04 | Fuel Pump Relay Control Circuit Open | ECM | DTC P0627 for the 2.0L diesel engine
P0627 54 | Fuel Pump Relay Control Circuit High Temperature | ECM | DTC P0627 for the 2.0L diesel engine
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P062B 03 | Control Module Fuel Injector Control Performance Voltage Below Threshold | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P062B 3B | Control Module Fuel Injector Control Performance Internal Self Test Failed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P062B 3C | Control Module Fuel Injector Control Performance Internal Communication Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P062F 36 | Control Module Long Term Memory Performance EEPROM Failure | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P062F 41 | Control Module Long Term Memory Performance Operational Software/Calibration Set Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L diesel engine
P0630 36 | VIN Not Programmed or Mismatched Engine Control Module (ECM) EEPROM Failure | ECM | DTC P0630 for the 2.0L diesel engine
P0630 47 | VIN Not Programmed or Mismatched Engine Control Module (ECM) VIN Not Programmed | ECM | DTC P0630 for the 2.0L diesel engine
P0641 03 | 5-Volt Reference 1 Circuit Below Threshold | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0641 07 | 5-Volt Reference 1 Circuit Above Threshold | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0642 or P0643 for the 2.0L and 2.5L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0643 | 5 Volt Reference 1 Circuit High Voltage | ECM | DTC P0642 or P0643 for the 2.0L and 2.5L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0646 for the automatic HVAC or DTC P0646 or P0647 for the manual HVAC
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0647 for the automatic HVAC or DTC P0646 or P0647 for the manual HVAC
P064C | Glow Plug Control Module Performance | ECM | DTC P064C for the 2.0L diesel engine
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650 for the 2.0L and 2.5L engine or DTC P0650 for the 2.0L diesel engine
P0650 01 | Malfunction Indicator Lamp (MIL) Control Circuit Short to Battery | ECM | DTC P0650 for the 2.0L diesel engine
P0650 02 | Malfunction Indicator Lamp (MIL) Control Circuit Short to Ground | ECM | DTC P0650 for the 2.0L diesel engine
P0650 04 | Malfunction Indicator Lamp (MIL) Control Circuit Open Circuit | ECM | DTC P0650 for the 2.0L diesel engine
P0650 54 | Malfunction Indicator Lamp (MIL) Control Circuit Temperature High | ECM | DTC P0650 for the 2.0L diesel engine
P0651 03 | 5-Volt Reference 2 Circuit Below Threshold | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0651 07 | 5-Volt Reference 2 Circuit Above Threshold | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0652 | 5-Volt Reference 2 Circuit Low Voltage | ECM | DTC P0652 or P0653 for the 2.0L and 2.5L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0653 | 5-Volt Reference 2 Circuit High Voltage | ECM | DTC P0652 or P0653 for the 2.0L and 2.5L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0654 | Engine Speed Output Circuit | ECM | DTC P0654
P0655 | Engine Coolant Temperature Lamp Control Circuit | ECM | DTC P0655 for the 2.0L diesel engine
P0655 01 | Engine Coolant Temperature Lamp Control Circuit Short to Battery | ECM | DTC P0655 for the 2.0L diesel engine
P0655 02 | Engine Coolant Temperature Lamp Control Circuit Short to Ground | ECM | DTC P0655 for the 2.0L diesel engine
P0655 04 | Engine Coolant Temperature Lamp Control Circuit Open Circuit | ECM | DTC P0655 for the 2.0L diesel engine
P0655 54 | Engine Coolant Temperature Lamp Control Circuit Temperature High | ECM | DTC P0655 for the 2.0L diesel engine
P0656 | Fuel Level Output Circuit | ECM | DTC P0656
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660, P0661, or P0662 for the 2.0L and 2.5L engine
P0661 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0660, P0661, or P0662 for the 2.0L and 2.5L engine
P0662 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit High Voltage | ECM | DTC P0660, P0661, or P0662 for the 2.0L and 2.5L engine
P0670 01 | Glow Plug Control Module Control Circuit Short to Battery | ECM | DTC P0670 for the 2.0L diesel engine
P0670 02 | Glow Plug Control Module Control Circuit Short to Ground | ECM | DTC P0670 for the 2.0L diesel engine
P0670 04 | Glow Plug Control Module Control Circuit Open Circuit | ECM | DTC P0670 for the 2.0L diesel engine
P0670 54 | Glow Plug Control Module Control Circuit Temperature High | ECM | DTC P0670 for the 2.0L diesel engine
P0671 02 | Glow Plug 1 Control Circuit Short to Ground | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0671 04 | Glow Plug 1 Control Circuit Open Circuit | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0672 02 | Glow Plug 2 Control Circuit Short to Ground | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0672 04 | Glow Plug 2 Control Circuit Open Circuit | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0673 02 | Glow Plug 3 Control Circuit Short to Ground | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0673 04 | Glow Plug 3 Control Circuit Open Circuit | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0674 02 | Glow Plug 4 Control Circuit Short to Ground | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0674 04 | Glow Plug 4 Control Circuit Open Circuit | ECM | DTC P0671, P0672, P0673, or P0674 for the 2.0L diesel engine
P0683 | Glow Plug Control Module Communication Circuit | ECM | DTC P0683 for the 2.0L diesel engine
P0683 3A | Incorrect Component Installed | ECM | DTC P0683 for the 2.0L diesel engine
P0683 71 | Invalid Serial Data Received | ECM | DTC P0683 for the 2.0L diesel engine
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0689 or P0690 for the 2.0L and 2.5L engine
P068A | Engine Controls Ignition Relay Control Circuit | ECM | DTC P068A, P068B, or P2510 for the 2.0L diesel engine
P068B | Engine Controls Ignition Relay Control Circuit | ECM | DTC P068A, P068B, or P2510 for the 2.0L diesel engine
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0689 or P0690 for the 2.0L and 2.5L engine
P0697 03 | 5-Volt Reference 3 Circuit Below Threshold | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0697 07 | 5-Volt Reference 3 Circuit Above Threshold | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L diesel engine
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700 for the 2.0L and 2.5L engine or DTC P0700 for the 2.0L diesel engine
P0741 | Torque Converter Clutch (TCC) System Stuck Off | TCM | DTC P0741 or P0742 for the 6T40/6T45 automatic transmission
P0742 | Torque Converter Clutch (TCC) System Stuck On | TCM | DTC P0741 or P0742 for the 6T40/6T45 automatic transmission
P1138 | H02S Circuit High Voltage During Decel Fuel Cut-OFF (DFCO) Bank 1 Sensor 2 | ECM | DTC P1138 or P1158 for the 2.0L and 2.5L engine
P1158 | H02S Circuit High Voltage During Decel Fuel Cut-OFF (DFCO) Bank 2 Sensor 2 | ECM | DTC P1138 or P1158 for the 2.0L and 2.5L engine
P1224 | Fuel Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P1224 01 | Fuel Injector 1 Control Circuit Short to Battery | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P1227 | Fuel Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P1227 01 | Fuel Injector 2 Control Circuit Short to Battery | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P122A | Fuel Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P122A 01 | Fuel Injector 3 Control Circuit Short to Battery | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P1233 | Fuel Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P1233 01 | Fuel Injector 4 Control Circuit Short to Battery | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L diesel engine
P1320 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1320 for the 2.0L and 2.5L engine
P1446 | Pre-Catalyst Temperature Too Low During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D for the 2.0L diesel engine
P1447 | Pre-Catalyst Temperature Too High During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D for the 2.0L diesel engine
P161C | Tire Size Not Programmed | ECM | DTC P161C for the 2.0L diesel engine
P161E 01 | Glow Plug Positive Voltage Circuit | ECM | DTC P161E for the 2.0L diesel engine
P161F | Assembly Plant Mode Counter Not Programmed | ECM | DTC P161F for the 2.0L diesel engine
P1628 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC P1628
P1629 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1629
P1648 | Theft Deterrent Security Code Incorrect | ECM | DTC P1648
P1663 | Change Engine Oil Lamp Control Circuit | ECM | DTC P1663 for the 2.0L diesel engine
P1663 01 | Change Engine Oil Lamp Control Circuit Short to Battery | ECM | DTC P1663 for the 2.0L diesel engine
P1663 02 | Change Engine Oil Lamp Control Circuit Short to Ground | ECM | DTC P1663 for the 2.0L diesel engine
P1663 04 | Change Engine Oil Lamp Control Circuit Open Circuit | ECM | DTC P1663 for the 2.0L diesel engine
P1663 54 | Change Engine Oil Lamp Control Circuit Temperature High | ECM | DTC P1663 for the 2.0L diesel engine
P1691 | Engine Coolant Temperature (ECT) Output Circuit | ECM | DTC P1691 for the 2.0L and 2.5L engine or DTC P1691 for the 2.0L diesel engine
P1691 01 | Engine Coolant Temperature (ECT) Output Circuit Short to Battery | ECM | DTC P1691 for the 2.0L diesel engine
P1691 02 | Engine Coolant Temperature (ECT) Output Circuit Short to Ground | ECM | DTC P1691 for the 2.0L diesel engine
P1691 04 | Engine Coolant Temperature (ECT) Output Circuit Open Circuit | ECM | DTC P1691 for the 2.0L diesel engine
P1691 54 | Engine Coolant Temperature (ECT) Output Circuit Temperature High | ECM | DTC P1691 for the 2.0L diesel engine
P2002 | diesel Particulate Filter Low Efficiency | ECM | DTC P2002 for the 2.0L diesel engine
P2031 03 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit Voltage Below Threshold | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P2031 07 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit Voltage Above Threshold | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P2032 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit Low Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P2033 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit High Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033 for the 2.0L diesel engine
P2072 | Throttle Actuator Control (TAC) System Ice Blockage | ECM | DTC P2072 for the 2.0L and 2.5L engine
P2080 | Exhaust Gas Temperature (EGRT) Sensor 1 Performance | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2080 08 | Exhaust Gas Temperature (EGRT) Sensor 1 Signal Invalid | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2080 13 | Exhaust Gas Temperature (EGRT) Sensor 1 Voltage Low/High Temperature | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2080 14 | Exhaust Gas Temperature (EGRT) Sensor 1 Voltage High/Low Temperature | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2084 | Exhaust Gas Temperature (EGRT) Sensor 2 Performance | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2084 08 | Exhaust Gas Temperature (EGRT) Sensor 2 Signal Invalid | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2084 13 | Exhaust Gas Temperature (EGRT) Sensor 2 Voltage Low/High Temperature | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2084 14 | Exhaust Gas Temperature (EGRT) Sensor 2 Voltage High/Low Temperature | ECM | DTC P2080 or P2084 for the 2.0L diesel engine
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 or P2098 for the 2.0L and 2.5L engine
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 or P2099 for the 2.0L and 2.5L engine
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098 for the 2.0L and 2.5L engine
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099 for the 2.0L and 2.5L engine
P20E2 | Exhaust Gas Temperature (EGT) Sensor 1-2 Correlation | ECM | DTC P20E2 for the 2.0L diesel engine
P20E2 5A | Exhaust Gas Temperature (EGT) Sensor 1-2 Plausibility Failure | ECM | DTC P20E2 for the 2.0L diesel engine
P2101 | Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P2101, P2118, or P2119 for the 2.0L and 2.5L engine
P2119 | Throttle Closed Position Performance | ECM | DTC P2101, P2118, or P2119 for the 2.0L and 2.5L engine
P2120 03 | Accelerator Pedal Position (APP) Sensor 1 Circuit Voltage Below Threshold | ECM | DTC P2120, P2125, or P2138 for the 2.0L diesel engine
P2120 07 | Accelerator Pedal Position (APP) Sensor 1 Circuit Voltage Above Threshold | ECM | DTC P2120, P2125, or P2138 for the 2.0L diesel engine
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L and 2.5L engine
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L and 2.5L engine
P2125 03 | Accelerator Pedal Position (APP) Sensor 2 Circuit Voltage Below Threshold | ECM | DTC P2120, P2125, or P2138 for the 2.0L diesel engine
P2125 07 | Accelerator Pedal Position (APP) Sensor 2 Circuit Voltage Above Threshold | ECM | DTC P2120, P2125, or P2138 for the 2.0L diesel engine
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L and 2.5L engine
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L and 2.5L engine
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L and 2.5L engine
P2138 5A | Accelerator Pedal Position (APP) Sensor 1-2 Correlation Plausibility Failure | ECM | DTC P2120, P2125, or P2138 for the 2.0L diesel engine
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P2146 or P2149 for the 2.0L diesel engine
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P2146 or P2149 for the 2.0L diesel engine
P2226 03 | Barometric Pressure (BARO) Sensor Circuit Voltage Below Threshold | ECM | DTC P2226, P2228, or P2229 for the 2.0L diesel engine
P2226 07 | Barometric Pressure (BARO) Sensor Circuit Voltage Above Threshold | ECM | DTC P2226, P2228, or P2229 for the 2.0L diesel engine
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2226, P2228, or P2229 for the 2.0L diesel engine
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2226, P2228, or P2229 for the 2.0L diesel engine
P2297 | H02S Performance During Decel Fuel Cut-Off (DFCO) Bank 1 Sensor 1 | ECM | DTC P2297 or P2298 for the 2.0L and 2.5L engine
P2298 | H02S Performance During Decel Fuel Cut-Off (DFCO) Bank 2 Sensor 1 | ECM | DTC P2297 or P2298 for the 2.0L and 2.5L engine
P2299 5A | Brake Pedal Position-Accelerator Pedal Position Correlation Plausibility Failure | ECM | DTC P2299 for the 2.0L diesel engine
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.0L and 2.5L engine
P244A | Diesel Particulate Filter Differential Pressure Too Low | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P244B | Diesel Particulate Filter Differential Pressure Too High | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P244B 11 | Diesel Particulate Filter Differential Pressure Too High Above Maximum Threshold | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P244C | Catalyst Temperature Too Low During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D for the 2.0L diesel engine
P244D | Catalyst Temperature Too High During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D for the 2.0L diesel engine
P2452 03 | Diesel Particulate Filter Differential Pressure Sensor Circuit Voltage Below Threshold | ECM | DTC P2452, P2454, or P2455 for the 2.0L diesel engine
P2452 07 | Diesel Particulate Filter Differential Pressure Sensor Circuit Voltage Above Threshold | ECM | DTC P2452, P2454, or P2455 for the 2.0L diesel engine
P2453 | Diesel Particulate Filter Differential Pressure Sensor Performance | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2453 08 | Diesel Particulate Filter Differential Pressure Sensor Performance Signal Invalid | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2453 11 | Diesel Particulate Filter Differential Pressure Sensor Performance Above Maximum Threshold | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2453 12 | Diesel Particulate Filter Differential Pressure Sensor Performance Below Minimum Threshold | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2453 18 | Diesel Particulate Filter Differential Pressure Sensor Performance Signal Amplitude Less Than Minimum | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2453 55 | Diesel Particulate Filter Differential Pressure Sensor Performance Expected Number of Transitions/Events Not Reached | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2453 58 | Diesel Particulate Filter Differential Pressure Sensor Performance Incorrect Reaction After Event | ECM | DTC P244A, P244B, or P2453 for the 2.0L diesel engine
P2454 | Diesel Particulate Filter Differential Pressure Sensor Circuit Low Voltage | ECM | DTC P2452, P2454, or P2455 for the 2.0L diesel engine
P2455 | Diesel Particulate Filter Differential Pressure Sensor Circuit High Voltage | ECM | DTC P2452, P2454, or P2455 for the 2.0L diesel engine
P2458 | Diesel Particulate Filter Regeneration Time | ECM | DTC P2458 for the 2.0L diesel engine
P2458 54 | Diesel Particulate Filter Regeneration Circuit/Component Protection Time-Out | ECM | DTC P2458 for the 2.0L diesel engine
P2463 | Diesel Particulate Filter Soot Accumulation | ECM | DTC P2463 for the 2.0L diesel engine
P2463 11 | Diesel Particulate Filter Soot Accumulation Above Maximum Threshold | ECM | DTC P2463 for the 2.0L diesel engine
P2510 58 | Engine Controls Ignition Relay Control Circuit Incorrect Reaction After Event | ECM | DTC P068A, P068B, or P2510 for the 2.0L diesel engine
P2510 59 | Engine Controls Ignition Relay Control Circuit/Component Protection Time-Out | ECM | DTC P068A, P068B, or P2510 for the 2.0L diesel engine
P2533 | Ignition 1 Switch Circuit | ECM | DTC P2533 for the 2.0L diesel engine
P2533 06 | Ignition 1 Switch Circuit Short to Ground or Open | ECM | DTC P2533 for the 2.0L diesel engine
P253F | Engine Oil Life | ECM | DTC P253F for the 2.0L diesel engine
P2544 72 | Transmission Torque Request Circuit Alive Counter Incorrect/Not Updated | ECM | DTC P2544 for the 2.0L diesel engine
P2544 74 | Transmission Torque Request Circuit Value of Signal Protection Calculation Incorrect | ECM | DTC P2544 for the 2.0L diesel engine
P260E | Diesel Particulate Filter Regeneration Lamp Control Circuit | ECM | DTC P260E for the 2.0L diesel engine
P260E 01 | Diesel Particulate Filter Regeneration Lamp Control Circuit Short to Battery | ECM | DTC P260E for the 2.0L diesel engine
P260E 02 | Diesel Particulate Filter Regeneration Lamp Control Circuit Short to Ground | ECM | DTC P260E for the 2.0L diesel engine
P260E 04 | Diesel Particulate Filter Regeneration Lamp Control Circuit Open Circuit | ECM | DTC P260E for the 2.0L diesel engine
P260E 54 | Diesel Particulate Filter Regeneration Lamp Control Circuit Temperature High | ECM | DTC P260E for the 2.0L diesel engine
P2687 01 | Fuel Heater Relay Control Circuit Short to Battery | ECM | DTC P2687 for the 2.0L diesel engine
P2687 02 | Fuel Heater Relay Control Circuit Short to Ground | ECM | DTC P2687 for the 2.0L diesel engine
P2687 04 | Fuel Heater Relay Control Circuit Open | ECM | DTC P2687 for the 2.0L diesel engine
P2687 54 | Fuel Heater Relay Control Circuit High Temperature | ECM | DTC P2687 for the 2.0L diesel engine
P268A | Fuel Injector Calibration Data Not Programmed | ECM | DTC P268A for the 2.0L diesel engine
P2A01 | H02S Circuit High Voltage During Decel Fuel Cut-Off (DFC) Bank 1 Sensor 2 | ECM | DTC P2A01 or P2A04 for the 2.0L and 2.5L engine
P2A04 | H02S Circuit High Voltage During Decel Fuel Cut-Off (DFC) Bank 2 Sensor 2 | ECM | DTC P2A01 or P2A04 for the 2.0L and 2.5L engine
U0001 | High Speed Can Communication Bus | ECM/TCM | DTC U0001
U0073 | High Speed Communication Bus | ECM | DTC U0073
U0100 | Lost Communication With ECM/transmission control module (TCM) | ECM | DTC U0100-U0299
U0167 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC U0100-U0299
U1500 | CAN 2 (Sensor Cluster) Bus Communication Malfunction (Bus Off) | EBCM/ESC | DTC U1500
U2100 | CAN Bus Communication Malfunction (Bus Off) | EBCM/ESC | DTC U2100
U2105 | Lost Communication with ECM | EBCM/ESC/TCS | DTC U2105-U2199
U2106 | Lost Communication with TCM | EBCM/ESC/TCS | DTC U2105-U2199
U2142 | Lost Communication with Sensor Cluster | EBCM/ESC | DTC U2105-U2199
U2143 | Lost Communication with Steering Wheel Angle Sensor | EBCM/ESC | DTC U2105-U2199