For 1990-2009 cars

## Fluid and Lubricant Recommendations Except Holden

Application | Specification
--- | ---
Metric | English
Engine Oil

- Gasoline Engine - API SL (ILSAC GF-III) grade/SAE 5W-30or
- API SL (ILSAC GF-II) grade/SAE 10W-40

6.4 L

6.7 qt

- Diesel Engine - MB229.31, 5W-40 (ACEA C3)

6.2 L

6.6 qt

Engine Coolant

- Important: Do not mix types of coolant.

  Mixture of water and DEX-COOL® or good quality ethylene glycol base antifreeze (year-round coolant)

8.0 L

8.4 qt

Brake Fluid and Clutch Fluid

- DOT-4

0.5 L

0.53 qt

Power Steering System Fluid

- DEXRON® II D

1.1 L

1.2 qt

Automatic Transaxle

- Gasoline Engine -ESSO JWS 3309 US ATF

7.14 ± 0.15 L

7.5 ± 0.15 qt

- Diesel Engine - ESSO JWS 3309 US ATF

6.94 ± 0.15 L

7.33 ± 0.15 qt

Manual Transaxle

- Gasoline Engine - SAE 75W-90

1.6 L

1.78 qt

- Diesel Engine - SAE 75W-90

2.1 L

2.2 qt

Manual Transaxle Shift Linkage

- Multipurpose-type grease meeting requirements NLGI No. 1 or 2

as needed

Key Lock Cylinders

- Silicone lubricant

as needed

Automatic Transaxle Shift Linkage

- Engine oil

as needed

Clutch Linkage Pivot Points

- Engine oil

as needed

Floor Shift Linkage Points

- Engine oil

as needed

Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine oil
2. Multipurpose-type grease meeting requirements NLGI No. 1 or 2

as needed

Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges

- Engine oil

as needed

Weatherstripping

- Silicone grease

as needed

## Fluid and Lubricant Recommendations Holden

Application | Fluid/Lubricant
--- | ---
Engine Oil |

• | SAE 5W-30 or 10W-30

• | API SL or SM

• | ILSAC GF-3 or GF-4

Engine Coolant | DEX-COOL® or conforming to Holden specification number GM6277M
Brake Fluid | DOT-4
Clutch Fluid | DOT-4
Power Steering System Fluid | DEXRON® III
Automatic Transaxle - Aisin 55-51LE | ESSO JWS 3309 ATF or conforming to Holden specification number HN2414
Manual Transaxle | SAE 75W-90
Manual Transaxle Shift Linkage | Multipurpose-type grease meeting requirements NLGI No. 1 or 2
Key Lock Cylinders | Silicone Lubricant
Automatic Transaxle Shift Linkage | Engine Oil
Clutch Linkage Pivot Points | Engine Oil
Floor Shift Linkage Points | Engine Oil
Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine Oil
2. Multipurpose-type grease meeting requirements NLGI No. 1 or 2

Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine Oil
Weatherstripping | Silicone Grease