For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the return spring from the mount brace.
3. Remove the nut, the washer, and the pedal mounting shaft.
4. Remove the locking washer and the piston rod bolt.
5. Remove the clutch pedal from the vehicle.

### Installation Procedure

1. Install the clutch pedal to the mount brace. Make sure the return spring engages the notch on the rear of the clutch pedal.
2. Coat the piston rod bolt with multi-purpose grease.
3. Install the piston rod bolt and the locking washer.
4. Coat the pedal mounting shaft with multi-purpose grease.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the pedal mounting shaft, the washer, and the nut.

Tighten
Tighten the clutch pedal nut to 18 N·m (13 lb ft).

6. Connect the return spring to the mount brace.
7. Connect the negative battery cable.