For 1990-2009 cars

### Removal Procedure

1. Remove the front bucket seat from vehicle. Refer to Front Seat Replacement - Bucket .
2. Remove the screws and slide the back panel down to remove it.
3. Remove the each seat trim.
4. Disconnect the electrical connectors.
5. Remove the bolts and the seat back.

### Installation Procedure

1. Install the seat back onto the seat cushion.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front seat back bolts.

Tighten
Tighten the front seat back bolts to 45 N·m (33 lb ft).

3. Connect the electrical connectors.
4. Install the seat trims to its original position.
5. Install the back panel onto the seat with the screws.

Tighten
Tighten the front seat cover screws to 12 N·m (106 lb in).

6. Install the front bucket seat in the vehicle. Refer to Front Seat Replacement - Bucket .