For 1990-2009 cars

## Fastener Tightening Specifications Gasoline

Application | Specification
--- | ---
Metric | English
Coolant Pump Mounting Bolts - 2.0L | 20 N·m | 15 lb ft
Coolant Pump Mounting Bolts - 2.5L | 10 N·m | 89 lb in
Coolant Temperature Gage Sensor | 20 N·m | 15 lb ft
Fan Assembly Mounting Bolts | 4 N·m | 35 lb in
Fan Motor Nut | 3.2 N·m | 28 lb in
Fan Motor Retaining Screws | 4 N·m | 35 lb in
Radiator Retaining Bolts - 2.0L | 4 N·m | 35 lb in
Radiator Retaining Bolts - 2.5L | 14 N·m | 10 lb ft
Surge Tank Attaching Bolt | 8 N·m | 70 lb in
Thermostat Housing Mounting Bolts - 2.0L | 15 N·m | 11 lb ft
Thermostat Housing Mounting Bolts - 2.5L | 20 N·m | 15 lb ft
Transaxle Fluid Cooler Pipe Bolt | 2.5 N·m | 22 lb in

## Fastener Tightening Specifications Diesel

Application | Specification
--- | ---
Metric | English
A/C Condenser Retaining Bolt | 9 N·m | 80 lb in
Auxiliary Cooling Fan Assembly Bolt | 4 N·m | 35 lb in
Charge Air Cooler Retaining Bolt | 8.5 N·m | 75.2 lb in
Fuel Pipe - Common Rail Retaining Bolt | 10 N·m | 88.5 lb in
Injection Pump Sprocket Nut | 70 N·m | 51.6 lb ft
Main Cooling Fan Assembly Bolt | 4 N·m | 35 lb in
Radiator Upper Bracket Retaining Bolt | 14 N·m | 10.3 lb ft
Surge Tank Retaining Bolt and Nut | 5 N·m | 44 lb in
Thermostat Housing Bolts | 23 N·m | 17 lb ft
Timing Belt Idler Bolt | 52 N·m | 38.4 lb ft
Timing Belt Rear Cover Bolt | 11 N·m | 97.4 lb in
Transaxle Oil Cooler and Line Retaining Bolt | 10 N·m | 88.5 lb in
Water Pipe Retaining Bolt (M6) | 9 N·m | 79.7 lb in
Water Pipe Retaining Bolt (M8) | 20 N·m | 14.8 lb ft
Water Pump Tightening Bolt | 11 N·m | 97.4 lb in