For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. The relay is located in front of the blower motor.
3. Remove the instrument panel (I/P) storage compartment lower panel cover. Refer to Instrument Panel Storage Compartment Replacement.
4. Separate the relay from the connector.
5. Remove the screws with the high-blower relay.

### Installation Procedure

1. Install the screws with the high-blower relay.
2. Connect the electrical connector.
3. Install the I/P storage compartment lower panel cover. Refer to Instrument Panel Storage Compartment Replacement.