For 1990-2009 cars

### Removal Procedure

Note: Left-Hand Drive Shown, Right-Hand Drive Similar

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the cruise control switch.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the cruise control switch with the screws and tighten to 3 N·m (27 lb in).
3. Connect the negative battery.