For 1990-2009 cars

#### Special Tools

• | KM-508-A Remover/Installer

• | KM-307-B Removal Plate or equivalent

### Disassembly Procedure

1. Remove the control arm. Refer to Control Arm Replacement .
2. Remove the control arm rear bushing using a press, the KM-307-B (1), and a drift.
3. Remove the control arm front bushing using a press, the KM-508-A (1) and the KM-307-B (2).

### Assembly Procedure

1. Coat the control arm rear shaft with a multipurpose lubricant. Refer to Fluid and Lubricant Recommendations .
2. Press the control arm front bushing into the control arm using a press, the KM-508-A (1) and the KM-307-B . Center the bushing.
3. Coat the outside of the control arm front bushing and the inside of the control arm with a multipurpose lubricant. Refer to Fluid and Lubricant Recommendations .
4. Press the control arm front bushing into the control arm using a press, the KM-508-A (1), and the KM-307-B (2). Center the bushing.
5. Install the control arm. Refer to Control Arm Replacement .